

**Visual Fault Locator S207**

This is specially designed for field personnel who need an efficient and economical tool for fiber tracing, fiber routing and continuity checking in optical network.

**Features**

**Metal case, Rugged and durable**

**Low battery indication, to avoid leakage and wrong judgment**

**ESD protection design, Protect the LD effectively**

**Integrated case, to avoid the case intermediate broken**

**Re-changeable ceramic tube, to avoid returning to manufacturer for this small fault**

**Long battery life, up to 60 hours＠1mW**

**Specifications**

|  |  |
| --- | --- |
| Central Wavelength | 650nm±10nm (635nm can be required on request) |
| Emitter Type | FP-LD |
| Output Power (mw) | 1, 10, 20, 30, 50 |
| Optical Connector | 2.5mm universal connectorFor 1.25mm connectors, FC (Male)-LC (Female) convertor can be optional on customer’s requests  |
| Operating Model | Both CW and Pulse available  |
| Pulse Frequency  | 2~3Hz  |
| Power Supply  | 2 AA alkaline batteries  |
| Battery Operating Time  | 650nm@1mw ≥65hours650nm@10mw≥15hoursTest with Panasonic LR6 AA ALKALINE battery  |
| Operating Temperature (℃) | -10~+45  |
| Storage Temperature (℃) | -40~+70  |
| Dimension (mm)  | ￠15X210  |
| Weight(g) | 120(Without battery)  |