**Fiber Cleaver D3**

**Specifications**

|  |  |
| --- | --- |
| Fiber diameter | 125µm |
| Outercoat diameter | 0.25mm-0.9mm |
| Fiber type | Single tube fiber and Ribbon fiber (exchangeable) |
| Cleaved length | 5-20mm |
| Cleaved angle | ≤0.5° |
| blade life | 48000 |
| Mode | Semiautomatic |
| Fiber collector | Available  |
| Dimension | 59mm(W)×55(D)mm×49mm(H) |
| Weight | 260g |